{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["HydraGS"],"not_rendered":{"charts":0,"images":8,"macros":1,"external_links":0,"defined_names":11,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"HydraGS","index":0,"n_rows":35,"n_cols":19,"rows_kept":35,"cut":false,"hidden":false,"merged":[[5,7,5,10],[4,13,4,15],[0,5,0,11],[2,7,2,10],[3,7,3,10],[4,7,4,10]]}
[null,null,null,null,null,"Druckverlustberechnung"]
[]
[null,"Gas Art",null,null,"Erdgas H",null,"Projektdaten",null,null,null,null,null,"Sprache/Language"]
[]
[null,"Gas Temperatur (°C)",null,null,"15","°C"]
[null,"Anschlußdruck (Pa)",null,null,"2000","Pa"]
[null,"zulässiger Druckverlust (Pa)",null,null,"300","Pa",null,""]
[null,"Betriebsheizwert (kWh/m^3)",null,null,"10,6","kWh/m³"]
[]
[]
[null,"Strang","Folge- Anschluß","Folge- anschluß (Strang 1)","Folge- anschluß (Strang 2)","Nenn- belastung (kW)","Höhen- unter- schied (m)","Nennweite (DN)","T-Stück","Länge in (m)","90° Bögen (Anzahl)","Anzahl Anschlüsse","Kunden- Bauteil Druck- verlust Gas [Pa]","Kommentar","Druck- verlust Strang (Pa)","Summe Druck- verlust (Pa)"]
[null,"Versorgung",null,10,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"deutsch"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"english"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"français"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"italiano"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"nederlands"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"© Witzenmann GmbH",null,null,null," ",null,null,null,null,null," ",null,null,"Hydra GS - Stand","2014-11-07"]